include: herringbone.atf, bladeEnd=le, bladeSide1=high, bladeSide2=low, \
                          bladeSide1PSuffix=, bladeSide2PSuffix=_p, \
                          point1Suffix=, point2Suffix=2, \
                          face0Edge2=4, face0Edge4=5

include: herringboneAttributes.atf, periodicSignVertex=4, \
                                    opening=in, openingU=IN, openingT=In, \
                                    bladeEnd=le, bladeEndU=LE, \
                                    position=leading, positionT=Leading, \
                                    direction=Up

Attribute: Retained Vertices=16
# Specify boundary layer edge on both sides of blade.  If it is cutoff at both
# ends, then there are 2 boundary layers.  Otherwise, they will turn out to have the
# same master edge.
# format: edge number, vertex number (of vertex on blade), blade #
Attribute: Edge Distribution Model=Boundary Layer, 9, 5, 1
Attribute: Edge Distribution Model=Boundary Layer, 12, 9, 1
Attribute: Periodic Start Vertex Centered=15
