include: herringbone.atf, bladeEnd=te, bladeSide1=high, bladeSide2=low, \
                          bladeSide1PSuffix=, bladeSide2PSuffix=_p, \
                          point1Suffix=, point2Suffix=2, \
                          face0Edge2=4, face0Edge4=5

include: herringboneAttributes.atf, periodicSignVertex=4, \
                                    opening=out, openingU=OUT, openingT=Out, \
                                    bladeEnd=te, bladeEndU=TE, \
                                    position=trailing, positionT=Trailing, \
                                    direction=Down
