version4.0
Lines 1: 3 lines of characters identifying the run (max 72 characters/line)
Typical correlations file for multistage axial fan
Miller Wright Correlations


Line 2: Integers for data and correlations
i_loss   i_dev   i_ewb
 2       2        2

Line 3: Loss input data 
n_loss_bladerow  dummy
  1               1

Line 4: Empirical deviation data (i_loss = 2)
i_blrow  i_loss_type  f_loss(1) f_loss(2) f_loss(3) f_loss(4) f_loss(5) f_loss(6)
  1       11	    1.0	  1.0       1.0       1.0       1.0       1.0

Line 5: Deviation input data (i_dev = 2)
n_dev_bladerow    dummy
  1			1

Line 6: Empirical deviation data (i_dev = 2)
i_blrow  i_dev_type   f_dev(1) f_dev(2) f_dev(3) f_dev(4) f_dev(5) f_dev(6)
  1       11	    0.0	 0.0      0.0      0.0      0.0       0.0

Line 7: Blockage input data 
n_ewb_bladerow  dummy
1                 1

Line 8: Empirical blockage data
i_blrow i_ewb_type   f_ewb(1)   ...   ...      ....      ...    f_ewb(6)
1        11          1.0        1.0      1.0      1.0      1.0     1.0  


