LIBRARY:
  USER ROUTINE DEFINITIONS:
    USER ROUTINE: myheatsource
      Calling Name = pt_heat_source
      Library Name = pt_heat_source
      Library Path = ..
      Option = Particle User Routine
    END
  END
END
FLOW: Flow Analysis 1
  DOMAIN: Domain 1
    Coord Frame = Coord 0
    Domain Type = Fluid
    DOMAIN MODELS:
      BUOYANCY MODEL:
        Option = Non Buoyant
      END
      DOMAIN MOTION:
        Option = Stationary
      END
      MESH DEFORMATION:
        Option = None
      END
      REFERENCE PRESSURE:
        Reference Pressure = 1 [atm]
      END
    END
    FLUID DEFINITION: Air Ideal Gas
      Material = Air Ideal Gas
      Option = Material Library
      MORPHOLOGY:
        Option = Continuous Fluid
      END
    END
    FLUID DEFINITION: Water
      Material = Water
      Option = Material Library
      MORPHOLOGY:
        Option = Dispersed Particle Transport Fluid
      END
    END
    FLUID MODELS:
      COMBUSTION MODEL:
        Option = None
      END
      FLUID: Air Ideal Gas
        HEAT TRANSFER MODEL:
          Option = Thermal Energy
        END
      END
      FLUID: Water
        EROSION MODEL:
          Option = None
        END
        HEAT TRANSFER MODEL:
          Option = Particle Temperature
        END
      END
      HEAT TRANSFER MODEL:
        Option = Fluid Dependent
      END
      THERMAL RADIATION MODEL:
        Option = None
      END
      TURBULENCE MODEL:
        Option = Laminar
      END
    END
    FLUID PAIR: Water | Air Ideal Gas
      Particle Coupling = Fully Coupled
      INTERPHASE HEAT TRANSFER:
        Option = None
        PARTICLE USER SOURCE:
          Argument Variables List = Temperature,Thermal \
            Conductivity,Water.Mean Particle Diameter,Water.Particle Nusselt \
            Number,Water.Temperature
          Particle Coupling = Fully Coupled
          Particle User Routine = myheatsource
          Particle User Source Return Variables List = Source,Source \
            Coefficient with respect to Particle Variable,Source Coefficient \
            with respect to Fluid Variable
        END
      END
      MOMENTUM TRANSFER:
        DRAG FORCE:
          Option = Schiller Naumann
        END
        PRESSURE GRADIENT FORCE:
          Option = None
        END
        VIRTUAL MASS FORCE:
          Option = None
        END
      END
    END
  END
END
