#=======================================================================
# @(#) $Id$
#-----------------------------------------------------------------------
#
########################################################################
#  DEFAULT MATERIALS LIBRARY FOR CFX-5
########################################################################
#
#  This file contains the CCL description of the default materials supplied
#  as part of the CFX-5 installation. These are the commonly used material
#  definitions that are presented in CFX-Pre.
#
########################################################################
LIBRARY:

MATERIAL GROUP: Air Data
  Group Description = \
    Ideal gas and constant property air.  Constant properties are for \
    dry air at STP (0 C, 1 atm) and 25 C, 1 atm.
END
MATERIAL GROUP: Water Data
  Group Description = \
    Liquid and vapour water materials with constant properties.  Can \
    be combined with NASA SP-273 materials for combustion modelling. 
END
MATERIAL GROUP: Gas Phase Combustion
  Group Description = \
    Ideal gas materials which can be use for gas phase combustion. \
    Ideal gas specific heat coefficients are specified using the \
    NASA SP-273 format.  
END
MATERIAL GROUP: Real Gas Combustion
  Group Description = \
    Real gas materials which can be use for gas phase combustion. \
    Ideal gas specific heat coefficients are specified using the \
    NASA SP-273 format.  
END
MATERIAL GROUP: Liquid Phase Combustion
  Group Description = \
    Liquid and homogenous binary mixture materials which can be included \
    with Gas Phase Combustion materials if combustion modelling also \
    requires phase change (eg: evaporation) for certain components.
END
MATERIAL GROUP: Constant Property Gases
  Group Description = \
    Gaseous substances with constant properties.  Properties are \
    calculated at STP (0C and 1 atm).  Can be combined with NASA SP-273 \
    materials for combustion modelling.
END
MATERIAL GROUP: Calorically Perfect Ideal Gases 
  Group Description = \
    Ideal gases with constant specific heat capacity.  Specific heat \
    is evaluated at STP.
END
MATERIAL GROUP: IAPWS IF97 
  Group Description = \
    Liquid, vapour and binary mixture materials which use the IAPWS \
    IF-97 equation of state.  Materials are suitable for compressible \
    liquids, phase change calculations and dry steam flows.
END
MATERIAL GROUP: Constant Property Liquids
  Group Description = \
    Liquid substances with constant properties.
END
MATERIAL GROUP: CHT Solids
  Group Description = \
    Pure solid substances that can be used for conjugate heat transfer.
END
MATERIAL GROUP: Particle Solids
  Group Description = \
    Pure solid substances that can be used for particle tracking
END
MATERIAL GROUP: Soot
  Group Description = \
    Solid substances that can be used when performing soot modelling 
END
MATERIAL GROUP: User
  Group Description = \
     Materials that are defined by the user
END
MATERIAL GROUP: Interphase Mass Transfer
   Group Description = \
     Materials with reference properties suitable for performing \
     either Eulerian or Lagrangian multiphase mass transfer problems.\
     Examples include cavitation, evaporation or condensation.
END
MATERIAL GROUP: Dry Redlich Kwong 
   Group Description = \
     Materials with properties specified using the built in \
     Redlich Kwong equation of state.  Suitable for dry real gas \
     modelling.
END
MATERIAL GROUP: Wet Redlich Kwong 
   Group Description = \
     Materials with properties specified using the built in \
     Redlich Kwong equation of state.  Suitable for wet real gas \
     modelling.
END
MATERIAL GROUP: Dry Soave Redlich Kwong 
   Group Description = \
     Materials with properties specified using the built in \
     Soave Redlich Kwong equation of state.  Suitable for dry real gas \
     modelling.
END
MATERIAL GROUP: Wet Soave Redlich Kwong 
   Group Description = \
     Materials with properties specified using the built in \
     Soave Redlich Kwong equation of state.  Suitable for wet real gas \
     modelling.
END
MATERIAL GROUP: Dry Peng Robinson
   Group Description = \
     Materials with properties specified using the built in \
     Peng Robinson equation of state.  Suitable for dry real gas \
     modelling.
END
MATERIAL GROUP: Wet Peng Robinson
   Group Description = \
     Materials with properties specified using the built in \
     Peng Robinson equation of state.  Suitable for wet real gas \
     modelling.
END
MATERIAL GROUP: Dry Steam
   Group Description = \
     Materials with properties specified using the IAPWS equation of \
     state.  Suitable for dry steam modelling.
END
MATERIAL GROUP: Wet Steam
   Group Description = \
     Materials with properties specified using the IAPWS equation of \
     state.  Suitable for wet steam modelling.
END
MATERIAL GROUP: Redlich Kwong Dry Steam
   Group Description = \
     Water materials which use the Redlich Kwong equation of state. \
     Suitable for dry steam modelling.
END
MATERIAL GROUP: Redlich Kwong Wet Steam
   Group Description = \
     Water materials which use the Redlich Kwong equation of state. \
     Suitable for condensing steam modelling.
END
MATERIAL GROUP: Redlich Kwong Dry Refrigerants
   Group Description = \
     Common refrigerants which use the Redlich Kwong equation of state. \
     Suitable for dry real gas models.
END
MATERIAL GROUP: Redlich Kwong Wet Refrigerants
   Group Description = \
     Common refrigerants which use the Redlich Kwong equation of state. \
     Suitable for condensing real gas models.
END
MATERIAL GROUP: Redlich Kwong Dry Hydrocarbons
   Group Description = \
     Common hydrocarbons which use the Redlich Kwong equation of state. \
     Suitable for dry real gas models.
END
MATERIAL GROUP: Redlich Kwong Wet Hydrocarbons
   Group Description = \
     Common hydrocarbons which use the Redlich Kwong equation of state. \
     Suitable for condensing real gas models.
END
MATERIAL GROUP: Soave Redlich Kwong Dry Steam
   Group Description = \
     Water materials which use the Soave Redlich Kwong equation of state. \
     Suitable for dry steam modelling.
END
MATERIAL GROUP: Soave Redlich Kwong Wet Steam
   Group Description = \
     Water materials which use the Soave Redlich Kwong equation of state. \
     Suitable for condensing steam modelling.
END
MATERIAL GROUP: Soave Redlich Kwong Dry Refrigerants
   Group Description = \
     Common refrigerants which use the Soave Redlich Kwong equation of state. \
     Suitable for dry real gas models.
END
MATERIAL GROUP: Soave Redlich Kwong Wet Refrigerants
   Group Description = \
     Common refrigerants which use the Soave Redlich Kwong equation of state. \
     Suitable for condensing real gas models.
END
MATERIAL GROUP: Soave Redlich Kwong Dry Hydrocarbons
   Group Description = \
     Common hydrocarbons which use the Soave Redlich Kwong equation of state. \
     Suitable for dry real gas models.
END
MATERIAL GROUP: Soave Redlich Kwong Wet Hydrocarbons
   Group Description = \
     Common hydrocarbons which use the Soave Redlich Kwong equation of state. \
     Suitable for condensing real gas models.
END
MATERIAL GROUP: Peng Robinson Dry Steam
   Group Description = \
     Water materials which use the Peng Robinson equation of state. \
     Suitable for dry steam modelling.
END
MATERIAL GROUP: Peng Robinson Wet Steam
   Group Description = \
     Water materials which use the Peng Robinson equation of state. \
     Suitable for condensing steam modelling.
END
MATERIAL GROUP: Peng Robinson Dry Refrigerants
   Group Description = \
     Common refrigerants which use the Peng Robinson equation of state. \
     Suitable for dry real gas models.
END
MATERIAL GROUP: Peng Robinson Wet Refrigerants
   Group Description = \
     Common refrigerants which use the Peng Robinson equation of state. \
     Suitable for condensing real gas models.
END
MATERIAL GROUP: Peng Robinson Dry Hydrocarbons
   Group Description = \
     Common hydrocarbons which use the Peng Robinson equation of state. \
     Suitable for dry real gas models.
END
MATERIAL GROUP: Peng Robinson Wet Hydrocarbons
   Group Description = \
     Common hydrocarbons which use the Peng Robinson equation of state. \
     Suitable for condensing real gas models.
END

END
