### 6.6.2. ExtrusionGuide

`class compolyx.ExtrusionGuide`(obj, parent=None)

Extrusion guide class

`active`

  Extrusion Guide active

`cad_geometry`

  Associated CADGeometry.

`depth`

  intensity for the propagation of mesh corrections, depth=1 leads to a linear decay from the guide to the radius, depth<1 leads to more local corrections

`direction`

  extrusion direction

`edge_set`

  Associated EdgeSet.

`radius`

  radius up to which nodal guide translations are propagated through the mesh

`use_curvature_correction`

  whether to use curvature correction algorithm to smooth mesh adapted to extrusion guide. Default is False

Release 18.2 - © ANSYS, Inc. All rights reserved.