#### 4.1.1.1. Workbench Integration

The Workbench Add-in of ACP installs two additional Component Systems to the Workbench Toolbox: ACP (Pre) and ACP (Post). These systems allow transferring the composite definitions of ACP between ACP and Mechanical on the Workbench schematic level. ACP is now fully integrated in the data structure of ANSYS Workbench and the update and refresh logic.

It is important that the user updates (refresh) the upstream data to pass the modifications to the ACP components. The update symbols can be used to check the up-to-date status of each component.

Release 18.2 - © ANSYS, Inc. All rights reserved.