### 3.4.4. General Application

The described features can also be used in combination with regular or woven materials and are not restricted to core materials. The selection of the method is often derived from the manufacturing process. Tabular values can be used for a winding process and CAD geometries for a CNC milling process. A Cut-off Selection Rule is often used in regions of sharp tapered edges (trailing edge of a wind turbine blade).

Release 18.2 - © ANSYS, Inc. All rights reserved.