#### 2.3.6.1. Export

Material data (Fabrics, Stackups and Sublaminates) and Sampling Points can be exported to ESAComp XML. A Fabric represents a Ply in ESAComp and Stackups, Sublaminates and Sampling Points are exported as Laminates.

To be sure that the imported values in ESAComp are in accordance to the ACP model, the FE import units in ESAComp should be checked first.

- Open FE import and export units in ESAComp.

- Adjust units in the Model Properties dialog (see ACP Model).

Release 18.2 - © ANSYS, Inc. All rights reserved.