### 2.1.3. Element and Edge Sets

Named selections defined in Mechanical or components defined Mechanical APDL can be imported into ACP. These selections are imported with the same names. Faces (element components in Mechanical APDL) are imported as Element Sets and edges (node components in Mechanical APDL) as Edge Sets.

Important: After the definition of a new Named Selection in Mechanical, the model must be updated.

Release 18.2 - © ANSYS, Inc. All rights reserved.