### 10.9.13. Parts - Zoning - Volume

This window lets you zone the interior volume of the IJK region you selected from nodes already defined on its six faces.

IJ-straight

  Select this option if you want to generate the interior volume so that nodes with the same (I,J) indices lie equally spaced along a straight line

JK-straight

  Select this option if you want to generate the interior volume so that nodes with the same (J,K) indices lie equally spaced along a straight line

IK-straight

  Select this option if you want to generate the interior volume so that nodes with the same (I,K) indices lie equally spaced along a straight line

Autozone

  Select this option if you want to generate the interior volume so that all nodes are spaced equipotentially.

Geometric Ratio

  Enter a geometric ratio in this field if you want to grade the zoning instead of equally spacing the nodes.

Release 18.2 - © ANSYS, Inc. All rights reserved.