### 5.14.6. Orthotropic Softening Model

To access local data

    USE matdef
    USE fai_orthodam

FT11 | Tensile Failure Stress 11
FT22 | Tensile Failure Stress 22
FT33 | Tensile Failure Stress 33
FT23 | Tensile Failure Stress 23
FT31 | Tensile Failure Stress 31
FT12 | Tensile Failure Stress 12
GF11 | Fracture energy 11
GF22 | Fracture energy 22
GF33 | Fracture energy 33
GF23 | Fracture energy 23
GF31 | Fracture energy 31
GF12 | Fracture energy 12
DCC | Damage Coupling Coefficient

Release 18.2 - © ANSYS, Inc. All rights reserved.