### 5.11.14. Compaction

To access local data

    USE matdef
    USE eos_compaction

RTBL`n` | Tabular density values, `n`= 1 to 10
PTBL`n` | Tabular pressure values, `n`= 1 to 10
For Linear unloading method
RTBL2`n` | Tabular density values (for soundspeed), `n`= 1 to 10
CTBL`n` | Tabular soundspeed values, `n`= 1 to 10
For Nonlinear unloading method
RTBL2`n` | Tabular density values (for Bulk Modulus), `n`= 1 to 10
CTBL`n` | Tabular Bulk Modulus values, `n`= 1 to 10

Release 18.2 - © ANSYS, Inc. All rights reserved.