### 5.14.3. Cumulative Failure Model

To access local data

    USE fai_cumdam

EPSZDA | Plastic strain at which damage starts to accumulate (also referred to as EPS1) | See Cumulative Damage Model in the Autodyn User's Manual
EPSMDA | Plastic strain at which damage reaches its maximum (also referred to as EPS2)
DAMMAX | Maximum damage, value between 0.0 and 1.0 (also referred to as Dmax)

Release 18.2 - © ANSYS, Inc. All rights reserved.