### 10.9.11. Parts - Zoning - Line

This window lets you generate nodes along a line in index space from its two end points. If either of its two end nodes has not been defined, you are asked to input the coordinates of the node.

I/J/K-varies

  The index direction of the line you want to generate. The line will be generated across the IJK range in the selected direction.

All

  Select this option if you want to generate nodes for all 12 edges of the IJK range you have specified.

Geometric Ratios

  Input geometric ratios in the fields provided if you want to grade the zoning instead of generating equally spaced nodes.

Line

  Select this option if you want to generate the nodes along a straight line.

Arc

  Select this option if you want to generate the nodes along the arc of a circle (you will be asked to specify the center of the circle).

Release 18.2 - © ANSYS, Inc. All rights reserved.