## 15.4. Detonation (2D) - Manual

This window lets you manually define initiation times for blocks of elements.

Part List

  Lists all the Parts in your model. Select the Part you want to define initiation time for in this list.

IJ range

  The IJ range for the block of elements to which you want to apply an initiation time.

Initiation time

  The initiation time that will be applied to all elements in the block.

Release 18.2 - © ANSYS, Inc. All rights reserved.