## Chapter 6: Autodyn Variable Listings

The Autodyn variables for structured 2D and 3D are listed below. The external output name is first given. This is the name shown on plots, printout, and when interactively examining values on the screen. The next column is the array name used internally. These internal names are to be used when writing user subroutines. Grid variables are either associated with a node (for example, X coordinate), or a cell center (for example, Pressure), or with a particle (SPH only). These are indicated as Node, Cell, and Particle respectively. Depending on the processor (solver), certain variables are not defined. This is indicated by a blank entry in the table.

The listings are provided for both versions 4 (Fortran 90) and versions 3 (Fortran 77).

Release 18.2 - © ANSYS, Inc. All rights reserved.