### 10.11.3. Parts - Boundary - Node

This window lets you apply a Boundary Condition to a node.

You cannot apply two different Velocity boundary conditions to structured beam parts.

IJK range for boundary

  The I, J, and K index for the node.

Boundary

  Select the boundary condition you want to apply from this pull-down menu.

  You can define Boundary Conditions by clicking the Boundaries button in the Navigation Bar, or you can click next to the pull-down menu.

Release 18.2 - © ANSYS, Inc. All rights reserved.