### 10.11.2. Parts - Boundary - I / J / K Plane

This window lets you apply a Boundary Condition to an I, J, or K plane of the current Part.

The example shown is for applying a Boundary Condition to an I plane (input for the other planes is similar).

You cannot apply two different Velocity boundary conditions to structured beam parts.

IJK range for boundary

  The I plane and the J and K range.

Boundary

  Select the boundary condition you want to apply from this pull-down menu.

  You can define Boundary Conditions by clicking the Boundaries button in the Navigation Bar, or you can click next to the pull-down menu.

Release 18.2 - © ANSYS, Inc. All rights reserved.