## 15.1. Detonation (2D) - Point

This window lets you define a detonation point.

X/Y Coordinates

  The X/Y coordinates of the detonation point.

Compute Initiation Time?

  Select whether you want to specify a detonation time, or have it computed by Autodyn.

  If selected, Autodyn will compute the detonation time using paths through the explosive from other detonation points.

  You must specify the initiation time for at least one detonation point, plane, cylinder or sphere.

Initiation Time

  The initiation time (unless you chose to have it computed).

Limit range of application?

  Limits the range of application of the detonation point (an extra dialog is presented).

Range will Include / Exclude region

  For each Part, you can specify an index range that is used to limit the range of application of the detonation point.

  Select whether you want the index range to specify the included region or the excluded region.

Part list

  Lists all the Parts in your model. Select a Part in this window to limit its range of application.

IJ range

  The IJ range you want to use to limit the range of application of the detonation point.

Release 18.2 - © ANSYS, Inc. All rights reserved.