### 10.11.1. Parts - Boundary - Block

This window lets you apply a boundary condition to a block in index space of the current structured Part.

For an unstructured Part the boundary condition will be applied to all nodes, elements or faces of a Part.

You cannot apply two different Velocity boundary conditions to structured beam parts.

IJK range for boundary

  The IJK range of the block.

Boundary

  Select the boundary condition you want to apply from this pull-down menu.

  You can define Boundary Conditions by clicking the Boundaries button in the Navigation Bar, or you can click next to the pull-down menu.

Release 18.2 - © ANSYS, Inc. All rights reserved.