### 5.11.11. Lee-Tarver EOS

To access local data

    USE matdef
    USE eos_leetarver

EZIG | Chapman-Jouguet(C-J) energy / unit volume in JWL EOS
A | A parameter
B | B parameter
R1 | R1 parameter
R2 | R2 parameter
W | W parameter
DETV | C-J detonation velocity
PCJ | C-J pressure
WREAC | Reaction zone width
DFMAX | Maximum change in reaction ratio
RRI | Ignition parameter I
RRB | Ignition reaction ratio exponent
RRA | Ignition critical compression
RRX | Ignition compression exponent
RRG1 | Growth parameter G1
RRC | Growth reaction ratio exponent c
RRD | Growth reaction ratio exponent d
RRY | Growth pressure exponent y
RRG2 | Growth parameter G2
RRE | Growth reaction ratio exponent e
RRG | Growth reaction ratio exponent g
RRZ | Growth pressure exponent z
FIGMAX | Maximum reaction ratio: ignition
FG1MAX | Maximum reaction ratio: growth G1
FG2MIN | Minimum reaction ratio: growth G2
LTUEOS | Unreacted Lee-Tarver EOS switch (shock, JWL)
VUMAX | Maximum relative volume in tension
SHKC0 | Parameter C1, unreacted shock EOS
SHKS | Parameter S1, unreacted shock EOS
SHKGAM | Gruneisen coefficient, unreacted shock EOS
AUR | Unreacted JWL, coefficient A
BUR | Unreacted JWL, coefficient B
R1U | Unreacted JWL, coefficient R1
R2U | Unreacted JWL, coefficient R2
WU | Unreacted JWL, coefficient W
EZIU | Unreacted JWL, internal energy / unit volume
VVNS | Unreacted JWL, Von Neumann spike volume

Release 18.2 - © ANSYS, Inc. All rights reserved.