### 36.4.6. Region Information

This section shows the names of the mesh regions that have been recognized as potential boundaries and interfaces. This name matching is done using the template names provided, which can be configured for your particular mesh files as appropriate. If the list of names that is shown is incorrect or incomplete, these can be modified accordingly. In the default case, this data should not need changing.

Turbo mode in CFX-Pre does not fully support meshes generated using the Line of rotation on hub and shroud setting in ANSYS TurboGrid. For meshes created using this setting, it may be necessary to manually adjust the regions selected under Region Information in order to obtain the correct interfaces and boundaries.

Release 18.2 - © ANSYS, Inc. All rights reserved.