## Chapter 26: User Locations

User locations enable you to specify an arbitrary set of points and connectivities that are not directly associated with the volume mesh, upon which the solver can write solution data. Post processing of these locations in CFD-Post provides a more efficient way to view data in regions of known interest and additionally can reduce the size of transient results files.

This chapter describes:

- User Surfaces
- Importing a User Surface into CFX-Pre

Release 18.2 - © ANSYS, Inc. All rights reserved.