### 13.2.3. Postprocessing

A successful ANSYS Multi-field run produces a CFX results file and a Mechanical application rst or rth file, which can be used to postprocess results. Both of these files can be postprocessed together by CFD-Post.

Specific information on CFD-Post's capabilities to read and use the Mechanical application results data can be found in ANSYS Files in the CFD-Post User's Guide.

The Mechanical application Post1 postprocessor can also be used to postprocess the Mechanical application results only.

Release 18.2 - © ANSYS, Inc. All rights reserved.