### 3.1.2. Example of Output Produced

If the export program is correctly compiled and run, the following output is obtained. For details, see Using a Customized Export Program.

In this example, the CFX results file contains three variables at user level 1: pressure, temperature and velocity. This is in a file named file.res. No timesteps or domains were specified, and the basename was specified as an example.

The following is displayed on screen:

    reading CFX results from <file.res>
    processing all domains
    writing Template Geometry file to <example.geom>
       writing 2365 nodes ... done
       writing 11435 elements... done
    writing Template results file to <example.res>
    writing variable output files
       Pressure    -> example.s01 ... done
       Temperature -> example.s02 ... done
       Velocity    -> example.v03 ... done

Five files are produced: the geometry file example.geom, the Template results file example.res, and three variable files called example.s01, example.s02 and example.v03, which contain the results for pressure, temperature and velocity, respectively. For details, see:

- example.geom

- example.res

- example.s01

#### 3.1.2.1. example.geom

The content of this file appears as:

    Template Geometry file exported from CFX
    node id given
    element id off
    coordinates
       2365
          1 2.00000e+00 0.00000e+00 0.00000e+00
          2-2.00000e+00-6.51683e-07 0.00000e+00
          3 2.00000e+00 0.00000e+00 2.00000e+00
          4-2.00000e+00-6.51683e-07 2.00000e+00
          5 3.00000e+00 1.00000e+00 5.00000e-01
          ....
          ....
          ....
          2362-1.13337e+00 2.18877e-01 4.02491e-01
          2363-1.12115e+00-3.66598e-01 2.22610e-01
          2364 1.36924e+00 4.78359e-01 1.22588e-01
          2365-3.30703e-01 1.38487e+00 2.23515e+00
    part 1
    volume elements
    tetra4
       11435
          754     230      12     145
          755     216       8     122
          756     212     125     215
          ....
          ....
          ....
          2365   496      475     474
    penta6
       0
    hexa8
       0

#### 3.1.2.2. example.res

The content of this file appears as:

    2 1 0
    1
    0.0
    0 1
    example.s01 Pressure
    example.s02 Temperature
    example.v03 Velocity

#### 3.1.2.3. example.s01

The content of this file appears as:

    Pressure
       1.42748e+04 1.42621e+04 1.43425e+04 1.43350e+04 1.44118e+04 1.44777e+04
       1.38639e+04 1.37352e+04 1.44130e+04 1.44755e+04 1.37733e+04 1.37626e+04
       ....
       ....
       ....
       1.39092e+04 1.40699e+04 1.24139e+04 1.34786e+04 1.34859e+04 1.37959e+04

Release 18.2 - © ANSYS, Inc. All rights reserved.