### 36.3.3. Analysis Type

The analysis type determines whether your problem is `Steady State`, `Transient`, or `Transient Blade Row`. If the problem is transient, set Total Time to the total simulation time and Time Steps to the timestep increment. For example, to study 10 timesteps over 0.1 seconds, set Total Time to `0.1 [s]` and Time Steps to `0.01 [s]`. If you choose the Transient Blade Row option under Analysis type, you have the option of choosing between the `Time Transformation` and `Fourier Transformation` methods under Methods.

For details, see Analysis Type.

Release 18.2 - © ANSYS, Inc. All rights reserved.