### 9.13.3. Initialization

The same initialization settings as for regular components can be set (that is, the default initial condition for NO of 0 mass fraction is appropriate for many configurations).

Tip: The NOx model can have problems if it is enabled for the first few iterations of a simulation. For improved robustness, obtain an established flow field first and then turn the NOx model on.

Release 18.2 - © ANSYS, Inc. All rights reserved.