### 7.13.2. Homogeneous Additional Variables in Multiphase Flow

Homogeneous Additional Variables are available for both homogeneous and inhomogeneous flow. However, in most cases, the homogeneous assumption is inappropriate for volumetric Additional Variables. For this reason, only specific Additional Variables are permitted to be homogeneous in ANSYS CFX.

Release 18.2 - © ANSYS, Inc. All rights reserved.