### 7.14.2. Bulk Sources

Bulk Sources automatically multiply the specified source by volume fraction, ensuring that the source reduces to zero as the fluid volume fraction reduces to zero. They can be used for equations that span all fluids as well as those that are fluid-dependent, such as mass fractions and Additional Variables. However, they may not be used for mass sources.

Release 18.2 - © ANSYS, Inc. All rights reserved.