### 18.4.4. Example of CCL File User Parameters

    USER:
    	#
    	# location of external inlet profiles.
    	InputFile = /home/cfxuser/u_profile.dat
    	#
    	# printing control switch.
    	User Printing = .FALSE.
    	#
    	# model option.
    	ModelOption = 1
    	#
    	# model data.
    	InletTemperature = 300
    	#
    	RadiusList = 0, 0.2, 0.4, 0.6, 0.8, 1
    	VelocityList = 1, 0.96, 0.84, 0.64, 0.36, 0
    END

Release 18.2 - © ANSYS, Inc. All rights reserved.