### 10.1.2. Convergence Tips

Sometimes, physical instabilities (such as recirculation zones) can result in slow or stalled convergence. In these cases, you can still obtain an indicator of convergence for a global quantity by creating a monitor point at some point in the domain. As a result, you can determine whether values for selected global quantities (such as gas hold-up) are meaningful.

Release 18.2 - © ANSYS, Inc. All rights reserved.