## Chapter 11: Analysis Type

The Analysis Type details view is used to specify whether the analysis requires coupling to an external solver, such as ANSYS Multi-field, and whether the analysis is steady-state, transient, or transient blade row. A discussion of external solver coupling is presented in Coupling CFX to an External Solver: ANSYS Multi-field Simulations in the CFX-Solver Modeling Guide. A discussion on steady-state and transient flows is presented in Steady State and Transient Flows in the CFX-Solver Modeling Guide.

Release 18.2 - © ANSYS, Inc. All rights reserved.