### 33.2.2. Details View for Termination Control

You access the details view for Termination Control from CFX-Pre by clicking Insert > Configurations > Termination Control or by right-clicking on Simulation Control in the details view and selecting Insert > Termination Control.

The following describes the details of the Termination Control tab.

Control Conditions

  A list displaying the available termination control conditions. Click Add new item to add a new termination control condition. To change its settings, the termination control condition must be highlighted. You can highlight a condition by selecting it from the displayed list. Click Delete to delete a highlighted termination control condition.

Control Condition: Options

  The options for termination control are either Max. Configuration Steps or Solver Interrupt Conditions. The former setting is used to terminate a simulations after a selected configuration has been executed the prescribed number of times. The latter setting is used to terminate a simulation whenever the named CFX-Solver interrupt conditions for the selected configurations have been satisfied. Note that the latter option is only valid if CFX-Solver interrupt conditions have been defined. For details, see Interrupt Control.

Control Condition: Configuration Name

  Choose the configuration for which the termination control is to be applied.

Control Condition: Number of Steps

  This setting is used to set to the maximum number of times the specified configuration is to be executed in the course of the simulation.

Control Condition: Condition Name(s)

  This setting is used to identify the names of the solver interrupt condition for the specified configuration to be used to terminate the simulation.

Release 18.2 - © ANSYS, Inc. All rights reserved.