## 9.3. Export to ANSYS MultiField Command

This option is used to produce files for use in Fluid Structure Interaction cases. For details, see Export to ANSYS Multi-field Solver Dialog Box.

1. Select Tools > Export to ANSYS MultiField.

   The Export to ANSYS MultiField Solver dialog box is displayed.

2. Under Results File, click Browse and select a results file for export.

3. If required, under Export File, click Browse and modify the default output path and name.

4. Under Domain Name, select the domain to export.

   Where multiple domains exist, select either one domain or all domains to export.

5. If required, under Boundary, select the boundaries to export.

6. Under Export Options, configure options as required.

   The options are dependent on the export type. For details, see Export to ANSYS Multi-field Solver Dialog Box.

7. Click Export.

   Once completed a message is displayed. Click OK to close it.

Release 18.2 - © ANSYS, Inc. All rights reserved.