### 15.5.6. Advection Schemes for Multiphase Volume Fractions

If you set the global advection scheme (that is, if you do not specify equation-class advection schemes) to upwind or high resolution, then the volume fraction equation will also be solved using upwind or high resolution. This is differs from ANSYS CFX-5.5.1 where upwind was always used for the volume fraction equations. However, if you set the global advection scheme to a specified blend, then the volume fraction equations will actually use the high resolution advection scheme but the maximum blend factor will be limited to the specified value instead of 1.

Release 18.2 - © ANSYS, Inc. All rights reserved.