### 5.12.2. Bulk Sources

Sources in multiphase flow often have the property that they scale with volume fraction, that is, as the volume fraction source goes to 0, the source also goes to 0. Bulk sources satisfy this property. They are applied at a fluid-independent level, and are therefore automatically added to the equations of all fluids for which they are relevant.

Release 18.2 - © ANSYS, Inc. All rights reserved.