## 8.6. Backup Run Command

Backing up a run creates a backup file of the results at the end of the timestep that is currently calculating. This file contains sufficient information for restarting a run for visualization. If a solution may be diverging and an intermediate solution must be retained, you should generate backup files.

To back up a run, either:

- Select Workspace > Backup Run.

- Click Backup Run .

The backup file is stored in a subdirectory within the working directory. This subdirectory is given the same name as the current run.

Release 18.2 - © ANSYS, Inc. All rights reserved.