## 9.8. Burning Velocity Model (Premixed or Partially Premixed)

This model is a combined model using:

- Model for the progress of the global reaction: Burning Velocity Model (BVM), also called Turbulent Flame Closure (TFC)

- Model for the composition of the reacted and non-reacted fractions of the fluid: Laminar Flamelet with PDF

The following topics will be discussed:

- Fluid Models

- Turbulent Burning Velocity

- Spark Ignition Model

- Boundary Settings

- Initialization

- Solver Parameters

- Other Parameters

Information on the theory behind this model is available in Burning Velocity Model (Premixed or Partially Premixed) in the CFX-Solver Theory Guide.

Release 18.2 - © ANSYS, Inc. All rights reserved.