### 8.4.1. Stopping Runs Using Mesh Adaption

If a stop current run command is issued for a run that uses mesh adaption, then only the current CFX-Solver run is terminated; the overall simulation, which includes equation solution and mesh adaption, is not. The CFX-Solver is automatically restarted after executing the next adaption step (if any remain), and the simulation continues.

Release 18.2 - © ANSYS, Inc. All rights reserved.