### 16.3.8. Results Options: Output Level

Availability: All Standard Formats (CGNS, MSC.Patran, FIELDVIEW and EnSight)

Default Value: 1.

The output level selects a predefined subset of variables to write to the destination results file. Each variable is given a “user level” by CFX-Solver. For details, see List of Field Variables.

An output level of:

- 1 writes a small subset of basic variables such as velocity and pressure, which have user level 1.

- 2 writes all variables that are of user levels 1 and 2.

- 3 writes all variables stored in the CFX results file.

Release 18.2 - © ANSYS, Inc. All rights reserved.