### 7.12.3. Turbulence Enhancement

In flows with a dispersed phase, large particles in the dispersed phase tend to increase turbulence in the continuous phase due to the presence of wakes behind the particles. This is known as particle induced turbulence. The `Sato Enhanced Eddy Viscosity` model can be used to model this effect. It is only available for fluid pairs using `Continuous` | `Dispersed` morphology. For details, see Fluid Pair Models Tab in the CFX-Pre User's Guide.

Release 18.2 - © ANSYS, Inc. All rights reserved.