## 1.13. Wall and Boundary Distance Formulation

Wall and boundary distances are used in various functions that control the transition between near-wall and freestream turbulence models, and in the mesh deformation model. These distances are derived using the same formulation, which is described here.

The following topics are discussed:

- 1D Illustration of Concept

- Concept Generalized to 3D

Release 18.2 - © ANSYS, Inc. All rights reserved.