## 8.8. Launching a New BladeEditor Model

A new BladeEditor model can be generated from an up-to-date Vista RTD system using the Create New > Geometry command in the right-click context menu of the Blade Design cell. This command launches ANSYS DesignModeler (with BladeEditor) and generates the new model.

Note: The DesignModeler model is detached from the Vista RTD system (that is, no link is generated). Therefore, any changes made to the Vista RTD system will not be reflected in the DesignModeler model following an update of the Vista RTD system.

Release 18.2 - © ANSYS, Inc. All rights reserved.