### 25.2.8. X-Z Plane Point

(applies only when Option is set to `Axis Points`)

In the reference Coordinate Frame, enter coordinates that define a point on the X-Z plane of the present Coordinate Frame.

The direction of this point from the nearest point on the Z axis is the direction of the X axis.

Tip: With Single Select selected, you may click locations in the viewer.

Release 18.2 - © ANSYS, Inc. All rights reserved.