7.12. Electronics server-mode jobs failing or not showing monitors

Engineering Knowledge Manager

EKM Troubleshooting Guide | Chapter 7: Job Management Issues |

7.11. MAPDL server-mode jobs failing, not showing live monitors, or can’t be paused |  | 7.13. Cannot run interactive jobs
Prev |  | Next

## 7.12. Electronics server-mode jobs failing or not showing monitors

When running a batch job using the Electronics job template, note the following:

- Electronics jobs will fail if submitted to a queue that uses a local scratch directory. Ensure that you select a queue that uses a shared scratch directory.

- Features introduced in current or recent releases of EKM may not be available in EKM if you choose a solver from an older release.

- When the DSO option is used, job monitoring during or after job execution is not available in EKM.

- Monitors remain displayed in the job view even after a job has been executed, or has failed. They do not remain displayed if you cancel the job.

Contains proprietary and confidential information of ANSYS, Inc. and its subsidiaries and affiliates.

Prev | Up / Contents | Next

Release 18.2 - © ANSYS, Inc. All rights reserved.