# This defines the attributes for the double herringbone topology for the
# leading or trailing edge of a single bladed system.

# has variables opening (in/out), openingU (IN/OUT), openingT (In/Out), 
#               bladeEnd (le/te), bladeEndU (LE/TE), 
#               position (leading/trailing), positionT (Leading/Trailing), 
#               direction (Up/Down)

Attribute: Periodic Sign=0, 1
Attribute: Domain Connection=[bladeEndU], 1, [bladeEnd]b1, [bladeEnd]2b1, [bladeEnd] focal minus, \
                             [bladeEnd] focal, [position] edgeb1
Attribute: Domain Connection=Local [direction]stream, [bladeEnd] focal
Attribute: Domain Connection=Global [openingT]let, [opening] ext
Attribute: Projection Object Map=Blade Centric,[bladeEnd]_focal_crv,[bladeEnd]_focal_minus_crv

include: cutoffBladeEndGeometry.atf, opening=[opening], openingU=[openingU], openingT=[openingT], \
                             bladeEnd=[bladeEnd], bladeEndU=[bladeEndU], \
                             position=[position], positionT=[positionT], \
                             direction=[direction]
